- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: AVN System / Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / AVN System / Description and Operation

Description

Limitations of the Navigation System
GPS Signal Reception State
As the GPS satellite frequency is received/transmitted in straight lines, reception may not work if hiding devices are placed on or near the GPS antenna or when traveling in the following locations.

• | Tunnels

• | Basement parking structures

• | Underneath an overpass

• | Roads within forested areas

• | Areas near high rise buildings

• | Roads within canyons

Vehicle Position Display

1. | If multipass errors occur due to reflections from buildings or related causes, the current position mark on the navigation may differ from the actual position of the vehicle.

2. | The position of the vehicle on the navigation may be different from the actual position if the vehicle is in the following status, however, this will automatically be adjusted by map matching or GPS information after driving a short distance. (This may take a several minutes in certain cases.)
• | When driving on a Y-shaped road with a narrow angle, the current position may be displayed in the opposite direction.
• | If the vehicle is loaded onto a car transport vehicle, the current position mark may be stalled on the last position prior to loading.
• | When driving on a spiral-shaped road.
• | When driving in mountainous regions with sharp turns or sudden brakes.
• | When entering a road after having been in an underground parking structure, building parking structure, or turntable with multiple rotations.
• | When the tires have recently been replaced (Especially upon use of spare or studless tires)
• | If the battery terminal is removed.
• | When driving in city streets, the current position may be displayed on the opposite side or on an off-road position.
• | When changing the zoom level from the maximum zoom in level to a different zoom level, the current position mark may be displayed on a different road.
• | When driving in heavy traffic with frequent stops or intersections.
• | When driving under slippery conditions, such as heavy sand, snow, etc.
• | When driving with tire chains installed.
• | When using a tire with an incorrect size specification.
• | When the tire pressures of all 4 tires are different from each other.
• | When the replacement tire is a worn or used tire (Especially studless tires having passed a 2nd seasons, etc.)
• | When driving near high-rise buildings
• | If a roof carrier has been installed
• | When driving under high speeds or having calculated a long-distance route.

Route Guidance
Suitable route guidance may not be available due to search conditions or driving conditions.

• | Guidance to go straight may be given while driving on a straight road.

• | Guidance may not be given even when having turned at an intersection.

• | There are certain intersections in which guidance may not occur.

• | In some cases, a route guidance may signal the driver to enter a no entry zone (No entry zone, road under construction, etc.)

• | Guidance may be given to a location near the actual destination if roads to the actual destination do not exist or are too narrow.

• | Wrong voice guidance may be given if the vehicle deviates from the designated route (e.g. If it turned at an intersection wherein the navigation guided to go straight.).

• | Missing or incorrect map data may cause unavailability of the route guidance.

Route Re-calculation
The following events may occur after conducting route recalculation.

• | Guidance may be given to a different position from the current position if the vehicle was turning at an intersection.

• | Route recalculation may take longer when driving under high speeds.

• | A route guidance signaling for a U-Turn in a No U-Turn zone may occur.

• | In some cases, a route guidance may signal the driver to enter a no entry zone (No entry zone, road under construction, etc.)

• | Guidance may be given to a location near the actual destination if roads to the actual destination do not exist or are too narrow.

• | Wrong voice guidance may be given if the vehicle deviates from the designated route (e.g. If it turns at an intersection wherein the navigation guided to go straight.).

##### Components and Components Location

Components Location 1. AVN (A/V & Navigation head unit)2. Tweeter speaker3. Roof antenna4. Front door speaker5. Rear door speaker6. Antenna feeder cable7. Back view camera8. Feeder cable join ...

##### AVN Head Unit Components and Components Location

Components AVN (A/V & Navigation) Head Unit Connector Connector Pin Information No.Connector AConnector BConnector C1Rear left speaker (+)MM CAN highC CAN (-)2Front left speaker (+)-C CAN ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: General Safety Information and Caution

Safety Precaution Since electric vehicles contain high voltage batteries, mishandling the high voltage system or vehicle may lead to a serious accident, including electric shock and electric leakage. • Be sure to shut o ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Shut-off Procedures

High Voltage Shut-off Procedure Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. ...
Copyright © www.ksoulev.com 2020-2021