- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Seat Belt / Rear Seat Belt Buckle Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Seat Belt / Rear Seat Belt Buckle Repair procedures

Replacement

[LH]

1. | Detach the rear seat belt lower anchor (C) by pushing the lock pin (B) of center mini buckle (A) with flat-tip driver.

2. | Remove the rear seat cushion assembly. (Refer to Rear Seat - "Rear Seat Assembly")

3. | Loosen the mounting bolt, and then remove the rear seat belt buckle [LH] (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.8 ~ 39.8 lb-ft)

4. | Install in the reverse order of removal.

[RH]

1. | Remove the rear seat cushion assembly. (Refer to Rear Seat - "Rear Seat Assembly")

2. | Loosen the mounting bolt, and then remove the rear seat belt buckle [RH] (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.8 ~ 39.8 lb-ft)

3. | Install in the reverse order of removal.

##### Rear Seat Belt Buckle Components and Components Location

Component Location 1. Rear seat belt buckle [LH]2. Rear seat belt buckle [RH] ...

##### Roof Trim

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Emergency Fastening Device (EFD) Repair procedures

Removal 1. Disconnect the battery negative cable, and wait for at least thirty seconds before beginning to work. 2. To remove the emergency fastening device (C), keep on pushing the lock pin (A) in the direction of arrow. And then remove the seat belt after pushing the lock pin (B). ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Steering Gear Rack, Linkage and Boots Repair procedures

Inspection 1. Check the steering wheel free road. (1) Turn the steering wheel so that the front wheels are facing straight ahead. (2) Measure the distance where the steering wheel can be turned without moving the front wheels. Standard value: 30mm (1.18in.) or less (3) If the pla ...
Copyright © www.ksoulev.com 2020-2021