- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Seat / Rear Seat Assembly Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Seat / Rear Seat Assembly Repair procedures

Replacement

[Rear seat back assembly]

1. | Detach the rear seat belt lower anchor (C) by pushing the lock pin (B) of center mini buckle (A) with flat-tip driver.

2. | Fold the rear seat back assembly.

3. | Remove the center hinge cover (A).

4. | Loosen the rear seat back mounting bolt (A).
Tightening torque : 16.7 ~ 25.5N.m (1.7 ~ 2.6kgf.m, 12.3~18.8lb-ft)

5. | Remove the rear seat back assembly (A).

6. | Install in the reverse order of removal.

[Rear seat cushion assembly]

1. | Remove the trunk trim.
(1) | Remove the luggage cover board (A).
(2) | Remove the luggage box (A).

2. | Remove the rear seat back[LH]. (Refer to Rear Seat - "Rear Seat Assembly")

3. | Loosen the rear seat cushion mounting bolt (A).
Tightening torque : 16.7 ~ 25.5N.m (1.7 ~ 2.6kgf.m, 12.3~18.8lb-ft)

4. | Remove the rear seat cushion assembly (A) by pushing it up.

5. | Disconnect the heater cushion connector (A). [LH] [RH]

6. | Install in the reverse order of removal.

##### Rear Seat Assembly Components and Components Location

Component Location 1. Rear seat back assembly [LH]2. Rear seat back assembly [RH]3. Rear seat cushion assembly ...

##### Rear Seat Back Cover Components and Components Location

Component Location 1. Rear seat back cover [LH]2. Rear seat back cover [RH] ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Quick-Charger Relay Assembly (QRA) Repair procedures

Removal QRA is integrated into the high voltage joint box and so each part cannot be replaced separately. Refer to removal procedure of high voltage joint box. Installation QRA is integrated into the high voltage joint box and so e ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Specifications

Specifications ItemSpecificationFront disc brakeTypeVentilated discDisc O.D.O 300 mm (11.81 in)Disc thickness28 mm (1.10 in)Caliper pistonSingleCylinder I.D.O 60.6 mm (2.36 in)Rear disc brakeTypeSolid discDisc O.D.O 284 mm (11.18 in)Disc thickness10 mm (0.39 in)Caliper pistonSingleCylinde ...
Copyright © www.ksoulev.com 2020-2021