- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Fender / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Fender / Repair procedures

Replacement

• | Be careful not to damage the fender and body.

• | When removing the clips, use a clip remover.

1. | Remove the head lamps. (Refer to Body Electrical System - "Head Lamps")

2. | Remove the A pillar garnish. (Refer to Body Side Moulding - "A Pillar Garnish")

3. | Remove the side sill moulding. (Refer to Body Side Moulding - "Side Sill Moulding")

4. | Using a clip remover, detach the clip, and remove the A pillar guard (A).

5. | Detach the clips and then remove the insulator pad (A).

6. | Loosen the front wheel guard mounting screws and bolt.

7. | Remove the front bumper side bracket (A) after loosening the screw and bolt.

8. | After loosening the mounting bolts and nuts, remove the fender assembly (A).

9. | Install in the reverse order of removal.
• | Make sure that the connectors are plugged in properly.
• | Replace any damaged clips.

##### Components and Components Location

Component Location 1. Fender assembly ...

##### Floor Carpet

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Runaway Arresting Device (RAD) Components and Components Location

Components Location 1. Runaway Arresting Device (RAD)2. Runaway Arresting Device (RAD) Wiring Harness ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Steering Gear box Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Loosen the bolt and then disconnect the universal joint assembly (A) from the pinion of the steering gear box. Tightening torque : 32.4 ~ 37.3N.m (3.3 ~ 3.8kgf.m, 23.9 ~ 27.5lb- ...
Copyright © www.ksoulev.com 2020-2021