- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / Inspection

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / Inspection

Inspection

When removing the battery pack assembly to inspect the battery system, it can be connected to vehicle by using the SST 0K918-E4100, 0K375-E4100, 0K375-E4200. Before installing the battery system assembly, check if the battery is OK by using the SST.

Insulation Resistance Loss Inspection

1. | Shut off the high voltage. (Refer to Battery Contorl System - "High Voltage Shut-off Procedure")

2. | Remove the high votlage battery upper case. (Refer to High Voltage Battery System - "Case")

3. | Remove the high voltage power cable (A).
High voltage power cable mounting nut : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)

4. | Measure the voltage between the high voltage power cable and the ground cable.
Specified value : Approx. 0 V

##### Schematic Diagrams

Circuit Diagram High Voltage Circuit Diagram ...

##### Battery Management System (BMS) ECU Specifications

Specification ItemSpecificationRemarkC-CAN terminating resistance (?)Approx. 60Combined resistance (BMS ECU-Inverter)C-CAN terminating resistnace (?)Approx. 120BMS ECU resistance ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components 1. Steering column assembly2. Universal joint assembly3. Steering gear box ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Adjustment 1. After loosening the tail gate hinge (A) mounting bolt, adjust the tail gate by moving it up and down, or right and left. 2. Adjust the tail gate height by turning the tail gate overslam bumpers (B). 3. After loosening the tail gate striker (C) mounting bolts, adjust the t ...
Copyright © www.ksoulev.com 2020-2021