- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Roof Trim / Sunvisor Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Roof Trim / Sunvisor Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Loosen the mounting screws, then remove the sunvisor (A) and retainer (B).

2. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Sunvisor Components and Components Location

Component Location 1. Sunvisor2. Retainer ...

##### Assist Handle Components and Components Location

Component Location 1. Assist handle ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High voltage joint box Repair procedures

Removal • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be sure ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Hub / Knuckle Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Remove the front wheel and tire (A) from front hub. Tightening torque: 88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft) Be careful not to da ...
Copyright © www.ksoulev.com 2020-2021