- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Cooling System / Cooling Fan Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Cooling System / Cooling Fan Repair procedures

Inspection

1. | Turn the ignition switch OFF and disconnect the auxiliary battery (12V) negative (-) terminal.

2. | Connect the GDS to DLC.

3. | Turn the ignition switch ON.

4. | Inspect "Control Duty" and waveforms according to "Fan Status" by performing "Actuation Test" on GDS.
Cooling Fan Speed | Duty (%) | Fan Speed (rpm)
0 | 0 | 0
1 | 10 | 900
2 | 20 | 1200
3 | 30 | 1500
4 | 40 | 1800
5 | 50 | 2100
6 | 60 | 2450
7 | 70 | 2600
8 | 80 | 2800
9 | 90 | 3000
[Cooling Fan at 1st Speed] [Cooling Fan at 2nd Speed] [Cooling Fan at 3rd Speed] [Cooling Fan at 4th Speed] [Cooling Fan at 5th Speed] [Cooling Fan at 6th Speed] [Cooling Fan at 7th Speed] [Cooling Fan at 8th Speed] [Cooling Fan at 9th Speed] [Cooling Fan Stop]

Removal

1. | Turn the ignition switch OFF and disconnect the auxiliary (12V) negative (-) terminal.

2. | Remove the rear cushion. (Refer to Body - "Rear Seat Assembly")

3. | After loosening the nut (A), remove the protector outlet duct panel (B).
Protector outlet duct panel mounting nut : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)

4. | Open the trunk.

5. | Remove the luggage board (A).

6. | After loosening the bolt (A), remove the outlet cooling duct (B).
Outlet cooling duct mounting bolt : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)

7. | After loosening the nut (A), remove the cooling fan (B).
Cooling fan mounting nut : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)

Installation

1. | Install in the reverse ordrer of removal.

##### Cooling Fan Description and Operation

Description It controls the BLDC motor speed by the PWM signal of BMS ECU. ...

##### Cooling Duct Description and Operation

Description It works as the air flow path when cooling fan operates. Battery Module Outlet Duct Protector Outlet Duct Panel Outlet Cooling Duct ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Audio Remote Control Components and Components Location

Components 1. Audio switch2. Cruise switch3. Bluetooth hands free switch4. Trip switch ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Receiver-Drier Repair procedures

Replacement [Without Heat Pump] 1. Remove the condenser, and then use an L wrench to remove the bottom cap (B) from the condenser. Tightening torque : 9.8 ~ 14.9 N.m (1.0 ~ 1.5 kgf.m, 7.2 ~ 10.8 lb-ft) 2. Remove the desiccant (A) from the condenser using a long nose plier. Che ...
Copyright © www.ksoulev.com 2020-2021