- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Heat Pump / 3-Way Coolant Valve Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Heat Pump / 3-Way Coolant Valve Repair procedures

Replacement

1. | Drain the coolant. (Refer to Traction Motor System - "Coolant")

2. | Disconnect the negative (-) battery terminal.

3. | Disconnect the 3-WAY solenoid coolant valve connector (A).

4. | Remove the 3-WAY coolant valve connector fixing clip (B).

5. | Remove the coolant hose (A) above 3-WAY coolant valve.

6. | Remove the coolant hose (A).

7. | Remove the 3-WAY coolant valve (B) after loosening the mounting bolts.

8. | Install in the reverse order of removal.

##### 3-Way Coolant Valve Description and Operation

Description Switches the valve outlet direction through electric signal to change refrigerant flow direction. Directs refrigerant flow towards chiller when heating pump is activated. Directs ref ...

##### Blower

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Crash Pad Lower Panel Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Panorama Sunroof Deflector Repair procedures

Replacement 1. Completely open the movable glass using the panorama sunroof switch. 2. Loosen he mounting screws (A) located at the side of the panorama sunroof deflector. • Be careful not to damage the screws. 3. Remove the panorama sunroof d ...
Copyright © www.ksoulev.com 2020-2021