- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Tire Pressure Monitoring System / TPMS Sensor Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Suspension System / Tire Pressure Monitoring System / TPMS Sensor Repair procedures

Removal

1. | Remove the tire. (Refer to Tires/Wheels - "Tire")

2. | Remove the screw with torx driver (A).
• | When installing the bead brake, make sure that it does not come in contact with the TPMS sensor.
• | Be careful not to damage the TPMS sensor when installing the bead brake near the TPMS sensor.

3. | Remove the sensor body (A) from the valve (B) in the direction of the arrow.

4. | Use the valve mounting tool to pull out the valve until it is entirely out of the lower hole.
Cut the rubber at the bottom of valve with a knife.

5. | Apply lubricant to the surface of the valve, and then mount it through the valve hole of the wheel.
We recommend using regular soapy water as lubricant.
• | The TPMS sensor valve bottom is not properly sealed if it is not fully mounted on the wheel, as shown in the following figure:
• | Make sure that the valve body is pulled entirely through the hole.

6. | Apply soapy water or lubricant to the upper/lower bead section of the tire.

7. | In order to mount lower the beads, place the TPMS sensor at 5 o''clock, starting from the head of the tire replacement equipment.

8. | Rotate the rim clockwise and press tire towards 3 o''clock to mount the lower beads.
• | Mount the tire on the wheel. Make sure that the beads touch the edge of the rim behind the sensor (towards 6 o''clock).

9. | In order to mount the upper beads, press the tire towards 3 o''clock and turn the rim clockwise.

10. | Inject air into the tire until the beads are in the correct position.

11. | Adjust the tire pressure according to the recommended tire pressure for the vehicle.

12. | If the TPMS sensor malfunctions, you must perform TPMS sensor learning. Replace any faulty sensors and perform TPMS sensor learning.

Diagnosis procedure by using diagnostic device

As manual for diagnosis methods by using diagnosis device, the main contents are as follows:

1. | Connect self-diagnosis connector(16pins) located in the lower of driver side crash pad to self-diagnosis device, and then turn the self-diagnosis device after key is ON.

2. | Select the "vehicle model" and "TPMS" on GDS vehicle selection screen, then select OK.

[System Identification (Wireless)]

[Sensor ID Writing (Wireless)]

[VIN input initialization]

[Vehicle name input initialization]

[Sensor Status initialization]

[Register Sensor initialization]

• | Write ID Read ID and be sure to check are the same.
• | After registering successfully sensor "Sensor Wireless Information" by the execution determines whether the sensor is working properly.

##### TPMS Sensor Description and Operation

Description Mode of Operation ASIC Mode 1. Factory Mode The factory mode is the mode that allows the TPM sensor to transmit RF Frames and sample LF more often in the HKMC factory. The TPM ...

##### TPMS Receiver Description and Operation

Description 1. Mode (1) Virgin State • The receiver as a sole part is shipped in this state. Replacement parts should therefore arrive in this state. • In this state, there ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: SRS Control Module (SRSCM) Repair procedures

Removal 1. Remove the ignition key from the vehicle. 2. Disconnect the battery negative cable and wait for at least three minutes before beginning to work. 3. Disconnect the DAB, PAB, SAB, CAB and BPT connectors. 4. Remove the floor console. (Refer to Body - "Floor console") 5. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Bumper Beam Assembly Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021