- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Suspension System / Front Lower Arm Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Suspension System / Front Suspension System / Front Lower Arm Repair procedures

Replacement

1. | Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported.

2. | Remove the front wheel and tire (A) from front hub.
Tightening torque: 88.3 ~ 107.9N.m (9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft)
• | Be careful not to damage to the hub bolts when removing the front wheel and tire (A).

3. | Remove the lower arm (A) from the knuckle.
Tightening torque: 58.9 ~ 70.6N.m (6.0 ~ 7.2kgf.m, 43.4 ~ 52.1lb-ft)

4. | Loosen the bolts (B,C), and then remove the front lower arm (A).
Tightening torque (B) 117.7 ~ 137.3N.m(12.0 ~ 14.0kgf.m, 86.8 ~ 101.3lb-ft) (C) 156.9 ~ 176.5N.m(16.0 ~ 18.0kgf.m, 115.7 ~ 130.2lb-ft)

5. | Installation is the reverse of removal.

Inspection

1. | Check the bushing for wear and deterioration.

2. | Check the front stabilizer bar for deformation.

3. | Check the all bolts and nuts.

##### Front Strut Assembly Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Remove the front wheel and tire (A) from front hub. Tightening torque: ...

##### Front Stabilizer Bar Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Loosen the bolt (A) and then disconnect the universal joint assembly from the pin ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Tail Gate Lift Repair procedures

Replacement • Take care to not let the tail gate fall on you as the lifts are removed. Have a helper hold the tail gate open, or use a secure method to hold it open. 1. Using a screwdriver (A), lift up slightly the socket clips (B) of both ends on ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Seat Frame Assembly Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021