- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Body Electrical System / Lighting System

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Lighting System

- Specifications
- Components and Components Location
- Head Lamps Components and Components Location
- Head Lamps Repair procedures
- Turn Signal Lamp Repair procedures
- Room Lamp Repair procedures
- Overhead Console Lamp Repair procedures
- Hazard Lamp Switch Repair procedures
- Rheostat Repair procedures
- Fog Lamps Repair procedures
- License Plate Lamps Repair procedures
- High Mounted Stop Lamp Repair procedures
- Luggage Lamp Repair procedures
- Rear Combination Lamp Repair procedures
- Sound Mood Lamp Components and Components Location
- Sound Mood Lamp Schematic Diagrams
- Sound Mood Lamp Repair procedures
- Charge Information Lamp Components and Components Location
- Charge Information Lamp Repair procedures
- Troubleshooting

##### Repair procedures

Inspection Front Door Lock Module Inspection 1. Remove the front door trim. (Refer to Body - "Front Door Trim") 2. Remove the front door module. (Refer to Body - "Front Door Module") 3. ...

##### Specifications

Specifications ItemsBulb Wattage (W)Bulb TypeFrontHead lamp (High)H7LL55Head lamp (Low)H7LL55Turn signal lampLEDLEDPosition lampLEDLEDFog lamp559006DRLLEDLEDSide marker5W5WSide repeater lamp (O/S ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Description and Operation

Heat Pump Configuration and Operation Heat pump is configured to circulate refrigerant flow for cooling/heating function. This process minimizes battery consumption by the heater resulting in enhanced driving distance of EV. [Heating] 1. Outer Condenser - Evaporates liquid refrigerant and f ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: TPMS Sensor Description and Operation

Description Mode of Operation ASIC Mode 1. Factory Mode The factory mode is the mode that allows the TPM sensor to transmit RF Frames and sample LF more often in the HKMC factory. The TPM sensor will send normal RF frames in factory mode. LF sampling will occur every 1 second, to ensu ...
Copyright © www.ksoulev.com 2020-2021