- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Horn / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Horn / Repair procedures

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove engine room under cover. (Refer to Motor System - "Under Cover")

3. | Remove the horn (A) after disconnecting the mounting bolt and connector.

Installation

1. | Install the horns after connecting the horn connectors.

2. | Install the engine room under cover.

Inspection

Test the horn by connecting the battery voltage to terminal 1 and the ground to terminal 2.
The horn should sound normally. If not, replace it.

##### Components and Components Location

Component Location 1. Horn switch2. Horn relay (EMS box)3. Horn 4. Clock spring ...

##### Indicators And Gauges

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Shut-off Procedures

High Voltage Shut-off Procedure Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Door Module Repair procedures

Replacement 1. Remove the front door window glass. (Refer to Front Door - "Front Door Window Glass") 2. Remove the front door outside handle. (Refer to Front Door - "Front Door Outside Handle") 3. Disconnect the front door main connector (A). 4. Loosen the front door outside handl ...
Copyright © www.ksoulev.com 2020-2021