- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Heating,Ventilation, Air Conditioning / High Voltage Shut-off Procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / High Voltage Shut-off Procedures

High Voltage Shut-off Procedure

Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries.

High voltage components : High Voltage Battery, Power Relay Assembly (PRA), Quick Charge Relay Assembly (QRA), Motor, Power Cable, BMS ECU, Inverter, LDC, On-Board Charger (OBC), Main Relay, Pre-charge Relay, Pre-charge resistor, Battery Current Sensor, Safety Plug, Main Fuse, Battery Temperature Sensor, Busbar, Charge Port, A/C Compressor, Electric Power Control Unit (EPCU), High Voltage Heater, High Voltage Heater Relay etc.

1. | Turn the ignition switch OFF and disconnect the negative (-) terminal of the auxiliary battery.

2. | Remove the cover (A) on the floor carpet of the rear seat.

3. | After loosening the nut, remove the safety plug service cover (A).
Safety plug service cover mounting nut : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)

4. | Remove the safety plug (A).
Remove the safety plug in the follwing order.

5. | Wait at least 5 minutes or until the capacitor in the high voltage system is fully discharged.

6. | Measure the voltage between the inverter terminals to check that the capacitor in the inverter is discharged completely
(1) | Lift the vehicle.
(2) | Remove the high voltage battery lower cover (A) by loosening the bolt.
(3) | Remove the high voltage cable (A).
(4) | Measure the voltage between the inverter terminals.
Less than 30 V : High voltage circuit properly shut More than 30 V : Faulty on high voltage circuit
If measured voltage is over 30V even though the safety plug has been removed properly, there may be a serious problem in the high voltage circuit. In this case, check DTC and never touch on the high voltage system.

##### General Safety Information and Caution

Safety Precaution Since electric vehicles contain high voltage batteries, mishandling the high voltage system or vehicle may lead to a serious accident, includi ...

##### Specifications

Specification Air Conditioner ItemSpecificationCompressorTypeESC33n (Electric Scroll)Communication typeCAN communicationOil type & CapacityPOE OIL, 180±10gMotor typeBLDCRated voltage360VOpe ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Specifications

Specification MotorJoint typeMax. permissible angleOuterInnerOuterInner80KWBJ#92TJ#9245°21° Tightening Torques ItemN.mkgf.mIb.ftFrontTire wheel hub nuts88.3 ~ 107.99.0 ~ 11.065.1 ~ 79.6Drive shaft coking nut274.6 ~ 294.228.0 ~ 30.0202.5 ~ 217.0Strut assembly to knuckle137.3 ~ 156.914.0 ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: ON-Board Charger (OBC) Specifications

Specification Maximum Output6.6kWOutput Density0.52kVA/?Size327 X 367 X 105 mmICCBApprox. 1.4kWEVSE6.6kW ...
Copyright © www.ksoulev.com 2020-2021