- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Door / Rear Door Module Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Door / Rear Door Module Repair procedures

Replacement

1. | Remove the rear door window glass. (Refer to Rear Door - "Rear Door Window Glass")

2. | Remove the rear door outside handle. (Refer to Rear Door - "Rear Door Outside Handle")

3. | After loosening the mounting bolt and nuts, remove the rear door channel (A).
Tightening torque : Bolt : 6.9 ~ 10.8 N.m (0.7 ~ 1.1 kgf.m, 5.1 ~ 8.0 lb-ft) Nut : 3.9 ~ 5.9 N.m (0.4 ~ 0.6 kgf.m, 2.9 ~ 4.3 lb-ft)

4. | Disconnect the rear door main connector (A).

5. | Loosen the rear door outside handle base mounting bolt (A).

6. | Loosen the rear door latch (A) mounting screws.

7. | After loosening the mounting bolts, remove the rear door module (B).
Tightening torque : Bolt : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft) Screw : 7.8 ~ 10.8 N.m (0.8 ~ 1.1 kgf.m, 5.8 ~ 8.0 lb-ft)

8. | Remove the rear door main connector mounting clips (A).

9. | Remove the rear door module wiring harness mounting clips (A).

10. | Disconnect the rear door latch connector (A) and then remove the mounting clip (B).

11. | Disconnect the connectors and rear door module wiring harness (A).

12. | Remove the rear door latch assembly. (Refer to Rear Door - "Rear Door Latch")

13. | Remove the rear speaker. (Refer to Body Electrical System - "Speakers")

14. | Remove the rear power window motor. (Refer to Body Electrical System - "Power Window Motor")

15. | Install in the reverse order of removal.
• | Apply sufficient grease on all rolling friction parts and springs.
• | Make sure that connectors are connected properly and each rod is connected securely.
• | Make sure that the door locks/unlocks and opens/closes properly.

##### Rear Door Module Components and Components Location

Component Location 1. Rear door module ...

##### Rear Door Outside Handle Components and Components Location

Component Location 1. Rear door outside handle ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Power Electric Frame Repair procedures

Removal 1. Remove the motor & gear drive unit. (Refer to Traction Motor System - "Motor & Gear Differential Unit Assembly") 2. Remove the Electric Water Pump (EWP). (Refer to Traction Motor System - "Electric Water Pump") 3. Remove the accumulator mounting bolt (A). Tighteni ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage PTC Heater Description and Operation

Operation Condition 1. The power supplied to the PTC heater should be within DC 240V - 420V (high voltage). 2. The power supplied to the PTC heater should be within 9.0V - 16.0V (low voltage). 3. The interlcok and insulation resistance must be normal. 4. The engine must be running. ...
Copyright © www.ksoulev.com 2020-2021