- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Suspension System / Sub Frame Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Suspension System / Front Suspension System / Sub Frame Repair procedures

Replacement

1. | Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported.

2. | Loosen the bolt (A) and then disconnect the universal joint assembly from the pinion of the steering gear box.
Tightening torque: 32.4 ~ 37.3N.m (3.3 ~ 3.8kgf.m, 23.9 ~ 27.5lb-ft)
Insert to the shaft in order that the center of the bolt and the marking (A) is in a straight line.

3. | Remove the front wheel and tire (A) from front hub.
Tightening torque : 88.2 ~ 107.8 N.m (9.0 ~ 11.0 kgf.m, 65.0 ~ 79.5 lb-ft)
• | Be careful not to damage to the hub bolts when removing the front wheel and tire (A).

4. | Remove the stabilizer link (A) loosening the nut.
Tightening torque : 98.1 ~ 117.7N.m(10.0 ~ 12.0kgf.m, 72.3~86.8lb-ft)

5. | Remove the tie rod end ball joint (C) from the knuckle by using the SST (09568-34000).
(1) | Remove the split pin (A).
(2) | Remove the castle nut (B).
(3) | Use the SST (09568-34000).
Tightening torque: 23.5 ~ 33.3N.m (2.4 ~ 3.4kgf.m, 19.4 ~ 24.6lb-ft)
• | When using SST, be sure not to damage the dust cover of lower arm ball joint.
• | Keep SST tied to the car because there is a risk of injury by dropping the SST during removing the lower arm ball joint.
• | The peripheral parts may be damaged when removing the lower arm ball joint with a general tool such as lever, so be sure to use SST.

6. | Loosen the bolt & nut and then remove the lower arm (A).
Tightening torque : 58.9 ~ 70.6 N.m (6.0 ~ 7.2 kgf.m, 43.4 ~ 52.1 lb-ft)

7. | Loosen the bolt and then separate the roll rod stopper (A).
Tightening torque : 107.9 ~127.5N.m(11.0 ~ 13.0kgf.m, 79.6 ~ 94.0lb-ft)

8. | Install the jack and then remove the bolt and nut.
Tightening torque Sub frame mounting bolts & nuts : 156.9 ~ 176.5N.m(16.0 ~ 18.0kgf.m, 115.7 ~ 130.2lb-ft)

9. | Remove the stabilizer (A) from the front sub frame by loosening the mounting bolts & nuts.
Tightening torque: 44.1 ~ 53.9N.m(4.5 ~ 5.5kgf.m, 32.5 ~ 39.8lb-ft)

10. | Remove the gear box (A) from the front sub frame by loosening the mounting bolts.
Tightening torque: 88.3 ~ 107.9N.m (9.0 ~ 11.0kgf.m, 43.4 ~ 57.9lb-ft)

11. | Remove the front lower arm. (Refer to Front Suspension System - "Front Lower Arm")

12. | Installation is the reverse of removal.

13. | Check the wheel Alignment. (Refer to Tires/Wheels - "Alignment")

##### Front Stabilizer Link Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Remove the front wheel and tire (A) from front hub. Tightening torque : 88.3 ...

##### Power Electric Frame Repair procedures

Removal 1. Remove the motor & gear drive unit. (Refer to Traction Motor System - "Motor & Gear Differential Unit Assembly") 2. Remove the Electric Water Pump (EWP). (Refer to Tractio ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Suspension Ball Joints Repair procedures

Inspection 1. Check the suspension ball joint. Check the grease leaks, kinks or damage in the front lower arm ball joint. 2. Check the grease leaks, kinks or damage in the tie rod end ball joint. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Center Pillar Trim Components and Components Location

Component Location 1. Center pillar lower trim2. Center pillar upper trim ...
Copyright © www.ksoulev.com 2020-2021