- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Hood / Hood Lift Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Hood / Hood Lift Repair procedures

Replacement

• | When removing and installing the hood lifter, work in a group of two or more.
• | When removing the clips, use a clip remover.

1. | Using a screwdriver (A), lift the socket clips (B) up slightly on both ends of the lifter (D), and then remove the lifter from the bracket (C).

2. | Push the socket of the lifter into the bracket for installation.
• | Make sure that the hood locks/unlocks and opens/closes properly.

##### Hood Assembly Repair procedures

Replacement • Be careful not to damage the hood and body. • When removing and installing the hood, work in a group o ...

##### Hood Insulator Pad Repair procedures

Replacement 1. Using a clip remover, detach the clips, and remove the hood insulator pad (A). • Be careful not to scratch the hood panel. 2. Install ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Crash Pad Center Panel Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Side Impact Sensor (SIS) Description and Operation

Description Side Impact Sensor (SIS) system consists of two P-SIS, installed at each center of front door modules (LH and RH), and two SIS, installed at each center of nearby pillars (LH and RH). P-SIS or Pressure Side Impact Sensor detects pressure due to collision at its mounting location. ...
Copyright © www.ksoulev.com 2020-2021