- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / Battery Current Sensor Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / Battery Current Sensor Specifications

Specifications

Current (A) | Ouput Voltage (V)
-400(Charge) | 0.5
-200 (Charge) | 1.5
0 | 2.5
200 (Discharge) | 3.5
+400 (Discharge) | 4.5

Item | Specifications | Remark
Current Sensor Output Voltage (V) | Approx. 2.5 ± 0.1 | Checkable by multi tester
Current Sensor Power Voltage (V) | Approx. 5 ± 0.1 | Checkable by multi tester

##### Pre-Charge Registor Repair procedures

Removal Main Relay, Pre Charge Relay, Pre Charge Resistor, Battery Current Sensor, High Voltage Battery Heater Relay and the High Voltage Battery Heater Fuse are in ...

##### Battery Current Sensor Description and Operation

Description Battery Current Sensor is installed in the Power Relay Assembly and it measures the current when the high voltage battery is being charged or discharged. [With High Voltage Batte ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Shut-off Procedures

High Voltage Shut-off Procedure Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Accumulator Repair procedures

Replacement 1. Recover the refrigerant with a recovery/ recycling/ charging station. • Do not use the same A/C recovery / charging station as conventional belt-driven compressors. • Since the electric compressor uses high-voltage, POE oil with ...
Copyright © www.ksoulev.com 2020-2021