- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Interior Trim / Cowl Side Trim Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Interior Trim / Cowl Side Trim Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the front door scuff trim. (Refer to Interior Trim - "Door Scuff Trim")

2. | Remove the hood latch release handle. (Refer to Hood - "Hood Latch Release Handle")

3. | Slighty remove the front door body side weatherstrip.

4. | Using a screwdriver or remover, remove the cowl side trim (A).

5. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Cowl Side Trim Components and Components Location

Component Location 1. Cowl side trim ...

##### Front Pillar Trim Components and Components Location

Component Location 1. Front pillar trim ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

General Inspection After or before servicing the EPS system, perform the troubleshooting and test procedure as follows. Compare the system condition with normal condition in the table below and if abnormal symptom is detected, perform necessary remedy and inspection. Test conditionNormal ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Cooling System Repair procedures

Inspection Radiator hoses 1. Check radiator hoses for the following (1) Improper attachment (2) Leaks (3) Cracks (4) Damage (5) Loose connections (6) Chafing (7) Deterioration Coolant level 1. Check the coolant level in the coolant reservoir. Make sure it is bet ...
Copyright © www.ksoulev.com 2020-2021