- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Power Train / Battery Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Maintenance / Power Train / Battery Repair procedures

Inspection

Battery Voltage and Status
Check the battery voltage and status using the battery tester.
Battery Terminal

1. | Move back and forth to check that the battery terminals (A) are loose or corroded. If the terminals are corroded, clean them.
If battery positive connection is loose, disconnect ground(GND) cable first before attempting to remove or tighten plus connection, to prevent personal injury.

2. | If the battery clamp on battery positive (+) terminal is not seated securely:
(1) | Turn ignition switch OFF and disconnect the battery negative (-) terminal.
(2) | Tighten battery clamp (A) on battery positive (+) terminal
Battery positive (+) terminal: 7.8 ~ 9.8 N.m (0.8 ~ 1.0 kgf.m, 5.8 ~ 7.2 lb-ft)

3. | If the battery clamp on battery negative (-) terminal is not seated securely:
(1) | Tighten battery clamp (A) on battery negative (-) terminal.
Battery negative (-) terminal: 4.0 ~ 6.0 N.m (0.4 ~ 0.6 kgf.m, 3.0 ~ 4.4 lb-ft)

Battery Condition
Check the battery for damage or deformation. If severe damage, deformation or leakage is found, replace the battery.

##### Power Train

...

##### Cooling System Repair procedures

Inspection Radiator hoses 1. Check radiator hoses for the following (1) Improper attachment (2) Leaks (3) Cracks (4) Damage (5) Loose connections (6) Chafing (7) Deterio ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Specifications

Specification ItemSpecificationRated voltageDC 3VOperating voltageDC 2.7V ~ 3.3VOperating temperature-20°C ~ +60°C (-4°F ~ +140°F)RF ModulationFSKLF ModulationASKRF frequency433.92 MHzBatteryCR2032 (3V / 1EA)Transmissible distance30m or moreBattery lifetime2 years or more (at 20 times per d ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Relay Box (Passenger Compartment) Description and Operation

Description Smart Junction Box(SJB) 1. General function : Interior Junction Box + some functions of BCM It uses CAN communication and IPS to control loads. 2. Main functions: – Low speed CAN communication (100kbps) – Self diagnosis (Lamp open/short) – Fail ...
Copyright © www.ksoulev.com 2020-2021