- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: SRSCM / SRS Control Module (SRSCM) Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / SRSCM / SRS Control Module (SRSCM) Description and Operation

Description

The primary purpose of the SRSCM (Supplemental Restraints System Control Module) is to determine an event that warrants restraint system air bag deployment. The SRSCM must decide whether to deploy the restraint system or not. After determining that pretensioners and/or airbag deployment is required, the SRSCM must supply sufficient power to the pretensioners and airbag igniters to initiate deployment.
The SRSCM determines whether or not an impact requires deployment of pretensioners and/or airbags based on data obtained from impact sensors and other components in conjunction with safety function.
The SRSCM will not be ready to detect a crash event or to activate the restraint system devices until the signals in the SRSCM circuitry are stabilized.
While it is possible that the SRSCM can activate the safety restraint devices, it is guaranteed to fully function after completing validation.
The SRSCM must perform a diagnostic routine and light a system readiness indicator at key-on. The system must perform a continuous diagnostic routine and provide fault annunciation through a warning lamp indicator in the event of fault detection. A serial diagnostic communication interface will be used to facilitate servicing of the restraint control system.
The yaw and G sensors which are used in ESC are located inside the SRSCM. The sensor signal is sent by a separate CAN signal between the ESC control module and SRSCM.

##### SRSCM

...

##### SRS Control Module (SRSCM) Components and Components Location

Components ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Disc Brakes and Pads Repair procedures

Inspection Check the pads for excessive wear, discs for run out and wear, and calipers for fluid leakage. Front Brake Front Brake Disc Thickness Check 1. Check the brake pads for wear and fade. 2. Check the brake disc for damage and cracks. 3. Remove all rust and contamination fro ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Normal Charge Cable Lock Actuator Repair procedures

Removal and Installation 1. Shut off the high voltage. (Refer to Battery Control System – “High Voltage Shut-off Procedure”) 2. Disconnect the auxiliary battery (12V) negative (-) terminal. 3. Disconnect the connector (A). 4. Remove the actuator by loosening the bolts (B). ...
Copyright © www.ksoulev.com 2020-2021