- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Heat Pump / 3-Way Coolant Valve Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Heat Pump / 3-Way Coolant Valve Description and Operation

Description

Switches the valve outlet direction through electric signal to change refrigerant flow direction.
Directs refrigerant flow towards chiller when heating pump is activated.
Directs refrigerant flow towards radiator during normal condition.

1. Towards radiator 2. Towards chiller 3. Inlet |

##### 3-Way Coolant Valve Components and Components Location

3-Way Coolant Valve 1. 3-Way Coolant Valve ...

##### 3-Way Coolant Valve Repair procedures

Replacement 1. Drain the coolant. (Refer to Traction Motor System - "Coolant") 2. Disconnect the negative (-) battery terminal. 3. Disconnect the 3-WAY solenoid coolant valve connector (A ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Sunvisor Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High voltage cable Repair procedures

Removal [High voltage battery pack - High voltage joint box] • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result ...
Copyright © www.ksoulev.com 2020-2021