- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Chassis / Brake Pedal Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Maintenance / Chassis / Brake Pedal Repair procedures

Inspection

Check that the brake pedal operates smoothly.
Brake Pedal Height and Stop Lamp Switch clearance Adjustment

1. | Disconnect the stop lamp switch connector (A).

2. | Adjust the brake pedal height (A) as illustration below.
Pedal height (A): 174.2 mm (6.86 in) Full stroke (C): 108 mm (4.25 in)

3. | Adjust the stop lamp switch clearance (B).
Stop lamp clearance (B): 1.0 ~ 2.0 mm (0.04 ~ 0.08 in)

4. | Connect the stop lamp switch connector

##### Brake Lines, Hoses and Connections Repair procedures

Inspection Visually check for proper installation, chafing, cracks, deterioration and any leakage Replace any deteriorated or damaged parts immediately. ...

##### Disc Brakes and Pads Repair procedures

Inspection Check the pads for excessive wear, discs for run out and wear, and calipers for fluid leakage. Front Brake Front Brake Disc Thickness Check 1. Check the brake pads for wear and fad ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Hood Latch Release Handle Repair procedures

Replacement 1. Using a screwdriver or remover, remove the hood release handle (A). • Use a 6mm hex bit to press the center until the handle easily pulls off the post. 2. Install in the reverse order of removal. • ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Audio Unit Components and Components Location

Components Connector Pin Information No.Connector AConnector B1Rear left speaker (+)-2Front left speaker (+)-3Front right speaker (+)-4Rear right speaker (+)Steering remocon5--6-USB D (+)7-USB/ iPod VDD8Illumination (+)AUX R input9DetentAUX ground10Rear left speaker (-)Mic (+) (Bluetooth)11Fro ...
Copyright © www.ksoulev.com 2020-2021