- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Steering wheel / Flex Steer Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Steering System / Steering wheel / Flex Steer Repair procedures

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Remove the driver airbag module. (Refer to Restraint - "Driver Airbag (DAB) Module and Clock Spring")

3. | Remove the steering wheel. (Refer to Steering System - "Steering Column and Shaft")

4. | Disengage the steering wheel remote control switch assembly. (Refer to Steering System - "Steering Wheel")

5. | Loosen the screw and then remote control switch assembly (A) from the steering wheel body.

6. | Install in the reverse order of removal.

##### Flex Steer Description and Operation

Instruction Flex Steer is system to choose the three modes power steering depending on driver preference or driving conditions. • Display on the cluster but p ...

##### Restraint

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Seat Belt Retractor Repair procedures

Replacement • When installing the belt, be careful not to damage the retractor. 1. Remove the rear pillar trim. (Refer to Interior Trim - "Rear Pillar Trim") 2. Loosen the rear seat belt upper anchor (A) mounting bolt. 3. After loosening the ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Shut-off Procedures

High Voltage Shut-off Procedure Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. ...
Copyright © www.ksoulev.com 2020-2021