- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: SRSCM / Occupant Detecting Sensor (ODS) Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / SRSCM / Occupant Detecting Sensor (ODS) Repair procedures

Removal

1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.

2. | Remove the front passenger seat assembly. (Refer to the Body group- Seat)

3. | Remove the seat cushion assembly. (Refer to the Body group- Seat)

Installation

1. | Install the ODS equipped seat cushion assembly. (Refer to the Body group- Seat)

2. | Install the front passenger seat assembly. (Refer to the Body group - seat)

3. | Reconnect the battery negative cable.

4. | After installing the ODS, confirm proper system operation :
• | Turn the ignition switch ON the SRS indicator should be turned on for about six seconds and then go off.
• | Telltale lamp will turn on for 4 seconds and be turned off for 3 seconds. After the 7 seconds, it shall remain off if the ODS does not require suppression and the passenger airbag is enabled.

##### Occupant Detecting Sensor (ODS) Components and Components Location

Components ...

##### Schematic Diagrams

Circuit Diagram (1) Circuit Diagram (2) Circuit Diagram (3) SRSCM Connector Terminal Harness Connector Pin No.Function (Connector A)Pin No.Function (Connector B)1--1--2--2--3--3--4- -4-- ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Battery Repair procedures

Inspection Battery Voltage and Status Check the battery voltage and status using the battery tester. Battery Terminal 1. Move back and forth to check that the battery terminals (A) are loose or corroded. If the terminals are corroded, clean them. If battery posi ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Power outlet relay2. Cooling fan relay 13. Defroster relay4. Cooling fan relay 25. EMS Box ...
Copyright © www.ksoulev.com 2020-2021