- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Interior Trim / Rear Pillar Trim Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Interior Trim / Rear Pillar Trim Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the luggage side trim. (Refer to Interior Trim - "Luggage Side Trim")

2. | After loosening the mounting bolts, remove the rear pillar trim (A).

3. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Rear Pillar Trim Components and Components Location

Component Location 1. Rear pillar trim ...

##### Mirror

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Stabilizer Bar Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Loosen the bolt (A) and then disconnect the universal joint assembly from the pinion of the steering gear box. Tightening torque: 32.4 ~ 37.3N.m (3.3 ~ 3.8kgf.m, 23.9 ~ 27.5lb-f ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Curtain Airbag (CAB) Module Repair procedures

Removal 1. Disconnect the battery negative cable and wait for at least thirty seconds before beginning to work. 2. Remove the roof trim assembly. (Refer to Body - "Roof trim assembly") 3. Disconnect the curtain airbag harness connector (A). 4. After loosening the mounting bolts and ...
Copyright © www.ksoulev.com 2020-2021