- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Electro Chromic Inside Rear View Mirror / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Electro Chromic Inside Rear View Mirror / Repair procedures

Inspection

Check the functions of the ECM in the following procedures:

1. | Turn the ignition key to the "ON" position.

2. | Cover the forward facing sensor.

3. | Flash a light onto the rearward looking sensor.

4. | The ECM should be darkened immediately on detecting light from the rearward looking sensor.
If this test is performed in daytime, the ECM may be darkened as soon as the forward facing sensor is covered.

5. | When the reverse gear is engaged, the ECM should not be darkened. When light is flashed onto both the forward facing and rearward looking sensors, the ECM should not be darkened.

Removal

1. | Remove the mirror wiring cover (A).

2. | Disconnect the ECM mirror connector (B).

3. | Loosen the mounting screw (B).

4. | Push the ECM mirror base up to remove the ECM mirror assembly (A).
Make sure not to damage the mounting bracket when removing the mirror.

Installation

1. | Install the mirror making sure that the mounting bracket is not damaged.

2. | Install the mirror wiring cover after reconnecting the connector and tightening the screw.
• | Make sure that the connectors are connected properly.
• | Replace any damaged clips.

##### Description and Operation

Description The Electro Chromatic inside rear view Mirror (ECM) is intended to dim the reflecting light in the rear view mirror. The forward facing sensor detects the brightness of the surround ...

##### Fuses And Relays

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Mounted Stop Lamp Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Remove the high mounted stop lamp trim (A). 3. Detach the high mounted stop lamp (A) from the tailgate after loosening the mounting bolts. 4. Remove the high mounted stop lamp (C) after disconnecting the connector (B) and ho ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Panorama Sunroof Motor Repair procedures

Inspection 1. Close the panorama sunroof glass and blind completely (Full close position). 2. Disconnect the negative (-) battery terminal. 3. Remove the roof trim assembly. (Refer to Body - "Roof Trim") 4. Remove the panorama sunroof glass motor (A) after loosening the screws and d ...
Copyright © www.ksoulev.com 2020-2021