- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Multifunction Switch / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Multifunction Switch / Repair procedures

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the steering wheel. (Refer to Steering System - "Steering Wheel")

3. | Remove the steering column upper and lower shrouds. (Refer to Body - "Steering Column Shroud Panel")

4. | Remove the clock spring. (Refer to Restraint - "Driver Airbag (DAB) Module and Clock Spring")

5. | Disconnect the light switch connector (A) and the wiper switch connector (B).

6. | Remove the wiper switch (A) by pushing the lock pin (B).
When removing the wiper & washer switch only, release the lock of wiper switch without removing the steering wheel.

7. | Loosen the screws from the multifunction switch assembly (A).

Installation

1. | Install the multifunction switch.

2. | Install the clock spring.

3. | Install the steering column upper and lower shrouds.

4. | Install the steering wheel.

5. | Connect the negative (-) battery terminal.
Make sure that the multifunction switch connectors are plugged in properly.

Inspection

Lighting Switch Inspection

1. | With the multifunction switch in each position, make sure that continuity exists between the following terminals. If continuity is not as specified, replace the multifunction switch. Lighting switch (Auto light) Lighting Switch Dimmer And Passing Switch Turn Signal Switch Front Fog Lamp

Wiper And Washer Switch Inspection

1. | With the multifunction switch in each position, make sure that continuity exists between the following terminals. If continuity is not as specified, replace the multifunction switch. Wiper Switch Washer Switch Rear Wiper Switch Rear Washer Switch

Inspection (With GDS)

1. | Check IPM input/output specification of multifunction switch using the GDS. If the specification is abnormal, replace the lamp or wiper switch.

2. | If diagnosis is required on the multifunction switch, select model and "IPM".

3. | Select "Current Data" to check the input/output conditions of "Multifunction switch".

4. | To perform test on "Multifunction switch" outputs, select "Actuation test".

##### Components and Components Location

Component ...

##### Panorama Sunroof

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Removal • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be sure ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Description and Operation

Description High Voltage Battery Control System High voltage battery control system consists of BMS ECU, PRA and it controls SOC (State of charge), output, trouble shooting, battery cell balancing, cooling, power supply & disconnect. Power Relay Assembly (PRA) consists of main relay ...
Copyright © www.ksoulev.com 2020-2021