- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Interior Trim / Door Scuff Trim Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Interior Trim / Door Scuff Trim Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Using a screwdriver or remover, remove the front door scuff trim (A). [Front]

2. | Remove the rear seat cushion assembly. (Refer to Rear Seat - "Rear Seat Assembly")

3. | Using a screwdriver or remover, remove the rear door scuff trim (A). [Rear]

4. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Door Scuff Trim Components and Components Location

Component Location 1. Front door scuff trim2. Rear door scuff trim ...

##### Cowl Side Trim Components and Components Location

Component Location 1. Cowl side trim ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Intake Actuator Repair procedures

Inspection 1. Turn the ignition switch OFF. 2. Disconnect the intake actuator connector. 3. Verify that the actuator operates to the recirculation position when 12V is connected to terminal 3 and ground to terminal 7. Verify that the intake actuator operates to the recirculated air posi ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: General Safety Information and Caution

Safety Precaution Since electric vehicles contain high voltage batteries, mishandling the high voltage system or vehicle may lead to a serious accident, including electric shock and electric leakage. • Be sure to shut o ...
Copyright © www.ksoulev.com 2020-2021