- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Lighting System / Luggage Lamp Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Lighting System / Luggage Lamp Repair procedures

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Using a screwdriver or remover, remove the luggage lamp (A).

3. | Remove the luggage lamp (A) after disconnecting the connector (B).

Installation

1. | Install the luggage lamp assembly after connecting the lamp connector.

##### High Mounted Stop Lamp Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Remove the high mounted stop lamp trim (A). 3. Detach the high mounted stop lamp (A) from the tailgate after loosening the mount ...

##### Rear Combination Lamp Repair procedures

Removal Rear Combination Lamp 1. Disconnect the negative (-) battery terminal. 2. Remove the rear combination lamp (A) after loosening the mounting screws. 3. Disconnect the rear combinat ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Power Door Lock Switch Repair procedures

Diagnosis With GDS 1. The BCM can be diagnosed by using the GDS. The BCM communicates with the GDS which then displays inputs and outputs along with codes. It will be able to quickly diagnose power door lock/unlock defects with GDS. GDS can operate the actuator forcefully, monitor input ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Description and Operation

Description BCM CAN Communication Function FunctionDescriptionTimerDefrosterWhen IGN ON, Rear Heater Control FunctionSafety Power WindowAccording to the position of key, Power Window Output ControlTailgateTailgate Open and Open Prohibition Control FunctionPanic AlarmUsing the RKE My Vehicle ...
Copyright © www.ksoulev.com 2020-2021