- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Seat / Front Seat Shield Outer Cover Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Front Seat / Front Seat Shield Outer Cover Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Using a driver or a remover, open and remove the height lever (B).

2. | Loosen the screw locking pin (A), and then remove the recliner lever (B).

3. | After loosening the screws, remove the shield outer cover (A).

4. | Install in the reverse order of removal.
• | Replace the damaged clip.

##### Front Seat Shield Outer Cover Components and Components Location

Component Location 1. Front seat shield outer cover ...

##### Front Seat Shield Inner Cover Components and Components Location

Component Location 1. Front seat shield inner cover ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Speaker Repair procedures

Inspection 1. Troubleshooting for Speaker (1) Basic inspection of speaker Inspect the sound from speaker after verifying that the speaker mounting screws are removed and the wiring connector is connected precisely to eliminate vibration transmitted from body trims and surrounding parts. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Charge Door Opener Actuator Switch Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Remove the crash pad lower panel. (Refer to Body - "Crash Pad Lower Panel") 3. Remove the crash pad lower switch assembly (A) by pushing it. 4. Disconnect the connector (A) from the crash pad lower switch assembly. 5. R ...
Copyright © www.ksoulev.com 2020-2021