- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Door / Front Door Side Weatherstrip Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Front Door / Front Door Side Weatherstrip Repair procedures

Replacement

1. | Loosen the front door checker (B) mounting bolt.
Tightening torque : 16.7 ~ 21.6 N.m (1.7 ~ 2.2 kgf.m,12.3 ~ 15.9 lb-ft)

2. | Detach the clips, and then remove the front door side weatherstrip (A).

3. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Front Door Belt Inside Weatherstrip Repair procedures

Replacement 1. Remove the front door trim. (Refer to Front Door - "Front Door Trim") 2. Remove the front door belt inside weatherstrip (A). 3. Install in the reverse order of removal. ...

##### Front Seat

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Virtual engine sound system unit2. Virtual engine sound speaker ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Console Armrest Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021