- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Towing / General Information

Kia Soul EV (PS EV) 2015-2020 Service Manual / General Information / Towing / General Information

Towing

If the vehicle needs to be towed, call a professional towing service. Never tow vehicle just on rope or a chain as It is very dangerous.
[Front]

[Rear]

Emergency Towing
There are three popular methods of towing a vehicle :

– | The operator loads the vehicle on the back of a truck. This is the best way of transporting the a vehicle.

– | The tow truck uses two pivoting arms that go under the tires of the driving axle and lift them off the ground. The other two wheels remain on the ground.

– | The tow truck uses metal cables with hooks on the ends. These hooks wrap around parts of the frame or suspension, and the cables lift that end of the vehicle off the ground. Attempting this method of towing can seriously damage the vehicle''s suspension and body.

If the vehicle cannot be transported by a flat-bed truck, it should be towed by lifting the wheels of the driving axle off the ground. In this case, the following procedure should be taken :
Reduction Gear Assembly

• | Start the motor.

• | Shift to [D] position, then [N] position.

• | Turn off the motor.

• | Improper towing preparation will damage the reduction gear assembly. Precisely the above procedure exactly. If you cannot shift the reduction gear or start the motor, your vehicle must be transported on a flatbed.
• | It is the best partice to tow the vehicle no farther than 30km (19miles), at a speed below 50km/h (30mph).
• | Trying to lift or tow your vehicle by the bumpers will cause serious damage. The bumpers are not designed to support the vehicle''s weight.

##### Towing

...

##### Warning And Caution Labels

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Crash Pad Lower Panel Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Hood Insulator Pad Repair procedures

Replacement 1. Using a clip remover, detach the clips, and remove the hood insulator pad (A). • Be careful not to scratch the hood panel. 2. Install in the reverse order of removal. • Replace any damaged clips ...
Copyright © www.ksoulev.com 2020-2021