- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Chassis / Brake Fluid Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Maintenance / Chassis / Brake Fluid Repair procedures

Inspection

1. | Check the brake fluid level.
Take care as brake fluid can harm your hands and eyes and damage painted surfaces. If fluid gets on your hands or in your eyes, flush the affected area with clean water immediately.
If brake fluid level is lower than the MIN line, check the clutch line or brake line for leaks and inspect the disc brake pads. If necessary, refill the reservoir with brake fluid to the MAX line after repair or replacement. Use the specified fluid. Avoid mixing different brands of fluid.
Specified fluid: SAE J1703 (DOT 3 or DOT 4)

##### Chassis

...

##### Brake Lines, Hoses and Connections Repair procedures

Inspection Visually check for proper installation, chafing, cracks, deterioration and any leakage Replace any deteriorated or damaged parts immediately. ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: PWM Blower Module Repair procedures

Inspection 1. Turn the ignition switch OFF. 2. Manually operate the control switch and measure the voltage of blower motor. 3. Select the control switch to raise voltage until high speed. Replacement 1. Disconnect the negative (-) battery terminal. 2. Remove the glove box housin ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Power Door Mirror Actuator Repair procedures

Inspection 1. Disconnect the negative (-) battery terminal. 2. Remove the front door quadrant cover (A). 3. Disconnect the power door mirror connector (A) from the harness. 4. Apply battery voltage to each terminal as shown in the table and verify that the mirror operates properly. ...
Copyright © www.ksoulev.com 2020-2021