- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Body Side Moulding / Roof Side Moulding Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Body Side Moulding / Roof Side Moulding Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Take care not to scratch the body surface.

1. | Using a screwdriver or remover, remove the roof side moulding (A).
• | Replace the roof side moulding with a new one.

2. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Body Side Moulding

...

##### Fender Garnish Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protec ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Floor Console Assembly Components and Components Location

Component Location 1. Floor console assembly ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Electric A/C compressor Troubleshooting

Troubleshooting Fault codeFail descriptionRemedy61Compressor CAN signal faultCompressor operation state error receive1. Check HV, LV connector connection. 2. Check LV connector pin condition. 3. Check vehicle inverter fuse condition. 4. A/C ON then check compressor operatio ...
Copyright © www.ksoulev.com 2020-2021