- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Seat / Rear Seat Latch Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Seat / Rear Seat Latch Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the rear seat back cover [LH]or [RH]. (Refer to Rear Seat - "Rear Seat Back Cover")

2. | After loosening the mounting bolts, then remove the rear seat latch (A).
Tightening torque : 19.6 ~ 29.4 N.m (2.0 ~ 3.0 kgf.m, 14.5 ~ 21.7 lb-ft)

3. | Remove the rear seat latch rod (A) to direction of the arrow.

4. | Install in the reverse order of removal.

##### Rear Seat Latch Components and Components Location

Component Location 1. Rear seat latch assembly ...

##### Rear Seat Folding Lever Components and Components Location

Component Location 1. Rear seat folding lever ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Rear glass defogger relay (Built-in smart junction box)2. Rear glass defogger switch (FATC type)3. Rear glass defogger ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Battery Temperature Sensor Repair procedures

Installation Battery temperature sensor can not be disassembled. 1. Turn the ignition switch OFF. 2. Shut off the high voltage. (Refer to Battery Control System - "High Voltage Shut-off Procedure") 3. Remove the high voltage battery system assembly. (Ref ...
Copyright © www.ksoulev.com 2020-2021