- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Identification Numbers / General Information

Kia Soul EV (PS EV) 2015-2020 Service Manual / General Information / Identification Numbers / General Information

Identification Numbers

Identification Number Description
Vehicle Identification Number

1. | World Manufacturer Identifier (WMI) - KNA : Passenger vehicle, MPV(Multipurpose Passenger Vehicle)/SUV(Sports Utility Vehicle)/RV(Recreational Vehicle) - KNC : Commercial vehicle (Van) - KND : MPV/SUV/RV (For U.S.A, Canada, Mexico) - KNH : Van

2. | Vehicle line - J : SOUL

3. | Model & Series - M : Low grade (L) - N : Middle-Low grade (GL) - P : Middle grade (GLS, JSL, TAX) - R : Middle-High grade (HGS)

4. | Body/Cabin type, Gross Vehicle Weight Rating KNA - 1 : Limousine - 2 : Sedan - 2 door - 3 : Sedan - 3 door - 4 : Sedan - 4 door - 5 : Sedan - 5 door - 6 : Coupe - 7 : Convertible - 8 : Wagon - 9 : Commercial Van - 0 : Pick-Up KNC (Commercial vehicle / Van) Except U.S.A, Canada, Mexico, Gulf Cooperation Council, China - X : Standard Cabin / Semi-Bonnet - Y : Double Cabin / Bonnet - Z : Super Cabin / Box For U.S.A, Canada, Mexico, Gulf Cooperation Council, China - 2 : Standard Cabin Class-H 4?2 - 3 : Standard Cabin Class-E 4?2 / Semi-Bonnet Class-E 4?2 - 4 : Standard Cabin Class-E 4?4 / Semi-Bonnet Class-E 4?4 - 5 : Standard Cabin Class-F 4?2 / Semi-Bonnet Class-F 4?2 - 6 : Standard Cabin Class-F 4?4 / Semi-Bonnet Class-F 4?4 - 7 : Double Cabin Class-E 4?2 / Bonnet Class-E 4?2 - 8 : Double Cabin Class-E 4?4 / Bonnet Class-E 4?4 - 9 : Double Cabin Class-F 4?2 / Bonnet Class-F 4?2 - 0 : Double Cabin Class-F 4?4 / Bonnet Class-F 4?4 - A : Super Cabin Class-E 4?2 / Box Class-E 4?2 - B : Super Cabin Class-E 4?4 / Box Class-E 4?4 - C : Super Cabin Class-F 4?2 / Box Class-F 4?2 - D : Super Cabin Class-F 4?4 / Box Class-F 4?4 KND - 1 : Wagon 4?2 Class-A - 2 : Wagon 4?2 Class-B - 3 : Wagon 4?2 Class-C - 4 : Wagon 4?2 Class-D - 5 : Wagon 4?2 Class-E - 6 : Wagon 4?2 Class-F - 7 : Wagon 4?2 Class-G - A : Wagon 4?4 Class-A - B : Wagon 4?4 Class-B - C : Wagon 4?4 Class-C - D : Wagon 4?4 Class-D - E : Wagon 4?4 Class-E - F : Wagon 4?4 Class-F - G : Wagon 4?4 Class-G KNH - 1 : Box - 2 : Bonnet - 3 : Semi-Bonnet

5. | Restraint system, Brake system KNA, KND Except U.S.A, Canada, Mexico - 0 : Both side - None - 1 : Both side - Active belt - 2 : Both side - Passive belt For U.S.A, Canada, Mexico
Code | Seat belt | Front air bag | Knee air bag | Side air bag | Curtain air bag
Driver''s | Passenger''s | Driver''s | Passenger''s | 1st row | 2nd row | 3rd row | 1st row | 2nd row | 3rd row
A | 0 | 0 | 0 | ? | ? | 0 | ? | ? | 0 | 0 | ?
B | 0 | 0 | 0 | ? | ? | ? | ? | ? | ? | ? | ?
C | 0 | 0 | 0 | ? | ? | 0 | ? | ? | 0 | 0 | 0
D | 0 | 0 | 0 | ? | ? | 0 | 0 | ? | 0 | 0 | ?
E | 0 | 0 | ? | ? | ? | ? | ? | ? | ? | ? | ?
F | 0 | 0 | 0 | ? | ? | 0 | ? | ? | ? | ? | ?
J | 0 | 0 | 0 | 0 | ? | 0 | 0 | ? | 0 | 0 | ?
L | 0 | 0 | 0 | 0 | ? | 0 | ? | ? | 0 | 0 | ?
N | 0 | ? | ? | ? | ? | ? | ? | ? | ? | ? | ?
H | 0 | 0 | 0 | 0 | ? | 0 | ? | ? | 0 | 0 | 0
KNC, KNH Except U.S.A, Canada, Mexico - 7 : Hydraulic brake system - 8 : Pneumatic brake system - 9 : Mixed brake system For U.S.A, Canada, Mexico - X : Hydraulic brake system - Y : Pneumatic brake system - Z : Mixed brake system

6. | Motor type - E : Battery [LiPB 350 V, 75 Ah] + Motor [3-phase AC 80 KW]

7. | Check digit or Driver’s side & Transmission Except U.S.A, Canada, Mexico, Gulf Cooperation Council, China, Yemen - A : LHD & MT - B : LHD & AT - C : LHD & MT+Transfer - D : LHD & AT+Transfer - E : LHD & CVT - F : LHD & Decelerator - G : LHD & DCT - L : RHD & MT - M : RHD & AT - N : RHD & MT+Transfer - S : RHD & AT+Transfer - T : RHD & CVT - U : RHD & Decelerator - V : RHD & DCT For U.S.A, Canada, Mexico, Gulf Cooperation Council, China, Yemen - Check digit : 0 ~ 9, ?

8. | Model year - E : 2014, F : 2015, G : 2016, H : 2017 …

9. | Production Plant - 5 : Hwaseong (Korea) - 6 : Soha-ri (Korea) - 7 : Gwangju (Korea) - T : Seosan (Korea)

10. | Vehicle production sequence number - 000001 ~ 999999

Motor Number

1. | Motor model

2. | Motor type - 80 : 80 KW

3. | Production year - D : 2013, E : 2014, F : 2015, G : 2016...

4. | Production month - 1 ~ 9 : January ~ September - A ~ C : October ~ December

5. | Production day For the motor produced before Nov. 2014 - 1 ~ 9 : 1st ~ 9th - A ~ V : 10th ~ 31st For the motor produced after Nov. 2014 (I, O, Q excluded) - 1 ~ 9 : 1st ~ 9th - A ~ Y : 10th ~ 31st

6. | Motor production sequence number - 001 ~ 999

7. | Vehicle line - N : SOUL EV

Paint Code

Code | Color
ACN | Snow White Pearl
AAT | Caribbean Blue
ABR | Cherry Black
IM | Titanium Silver
1D | Clear White

##### Identification Numbers

...

##### Lift And Support Points

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Special Service Tools

Special Service Tools Tool Name / NumberIllustrationDescriptionHog ring clip installer09880-4F000Used to install hog ring clip Personal Protective Equipment NameIllustrationDescriptionInsulation glovesUsed when inspecting or working on the high voltage components[Insulation performance : ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Brake Actuation Unit Repair procedures

Removal 1. Turn ignition switch OFF and disconnect the negative (-) battery cable. 2. Disconnect the brake fluid level switch connector (A), and remove the reservoir cap. Be sure to completely remove foreign substances around brake fluid reservoir and cap be ...
Copyright © www.ksoulev.com 2020-2021