- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Crash Pad / Crash Pad Side Cover Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Crash Pad / Crash Pad Side Cover Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

[LH]

1. | Using a screwdriver or remover, remove the crash pad side cover [LH] (A).

2. | Install in the reverse order of removal.
• | Replace any damaged clips.

[RH]

1. | Using a screwdriver or remover, remove the crash pad side cover [RH] (A).

2. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Crash Pad Side Cover Components and Components Location

Component Location [LH] 1. Crash pad side cover [LH] [RH] 1. Crash pad side cover [RH] ...

##### Crash Pad Center Panel Components and Components Location

Component Location 1. Crash pad center lower panel ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High voltage joint box Description and Operation

Description Function: The high voltage joint box distribute high voltage to the each unit of vehicle. High-voltage power charge / output system flow ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Seat Belt Buckle Switch (BS) Repair procedures

Removal 1. Disconnect the battery negative cable, and wait for at least three minutes before beginning work. 2. Remove the front seat assembly. (Refer to Body - "Front seat") 3. Remove the seat belt buckle switch. (Refer to Body - "Front seat belt buckle") Installation ...
Copyright © www.ksoulev.com 2020-2021