- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Restraint / Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / Specifications

Tightening Torque

Item | Nm | kgf.m | lb-ft
Passenger Airbag (PAB) | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.9 ~ 8.6
Curtain Airbag (CAB) | Bolt | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.9 ~ 8.6
Nut | 3.9 ~ 5.9 | 0.4 ~ 0.6 | 2.9 ~ 4.4
Side Airbag (SAB) | 5.9 ~ 7.8 | 0.6 ~ 0.8 | 4.3 ~ 5.8
SRSCM | 7.8 ~ 9.8 | 0.8 ~ 1.0 | 5.7 ~ 7.3
Front Impact Sensor (FIS) Mounting nut | 7.8 ~ 9.8 | 0.8 ~ 1.0 | 5.7 ~ 7.3
Pressure Side Impact Sensor (PSIS) Mounting Screw | 3.5 ~ 5.7 | 0.36 ~ 0.58 | 2.6 ~ 4.2
Side Impact Sensor (SIS) Mounting Bolt | 7.8 ~ 9.8 | 0.8 ~ 1.0 | 5.7 ~ 7.3

##### General Information

General The supplemental restraint system (SRS) is designed to supplement the seat belt to help reduce the risk or severity of injury to the driver and passenger by activating and deploying the ...

##### Components and Components Location

Components 1. Driver Airbag (DAB)2. Steering Wheel3. Clock Spring4. Seat Belt Pretensioner (BPT)5. Side Impact Sensor (SIS)6. Side Airbag (SAB)7. Passenger Airbag (PAB)8. Front Impact Sensor (FIS ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components 1. Windshield glass 2. Windshield glass moulding ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Seat Folding Lever Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021