- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: SRSCM / Front Impact Sensor (FIS) Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / SRSCM / Front Impact Sensor (FIS) Description and Operation

Description

The Front Impact Sensors (FIS) are installed in the Front End Module (FEM). These remote sensors are used to detect acceleration due to a collision at the mounting location.
The primary purpose of the Front Impact Sensor (FIS) is to provide an indication of a collision. The Front Impact Sensor (FIS) sends acceleration data to the SRSCM.

##### SRS Control Module (SRSCM) Repair procedures

Removal 1. Remove the ignition key from the vehicle. 2. Disconnect the battery negative cable and wait for at least three minutes before beginning to work. 3. Disconnect the DAB, PAB, SAB, ...

##### Front Impact Sensor (FIS) Components and Components Location

Components ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Instrument Cluster Description and Operation

Description Mian Features 1. Power and charge guage (1) It displays the degree of economic driving by identifying the status of a driver''s operation, depending on a vehicle''s driving conditions (e.g., required power, system efficiency and charging). (2) It leads to economic driving ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Specifications

Specification Air Conditioner ItemSpecificationCompressorTypeESC33n (Electric Scroll)Communication typeCAN communicationOil type & CapacityPOE OIL, 180±10gMotor typeBLDCRated voltage360VOperation voltage240~413VDisplacement33cc/revCondensorHeat rejection13,400 -3% kcal/hrAir pressure tran ...
Copyright © www.ksoulev.com 2020-2021