- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Door / Front Door Belt Inside Weatherstrip Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Front Door / Front Door Belt Inside Weatherstrip Repair procedures

Replacement

1. | Remove the front door trim. (Refer to Front Door - "Front Door Trim")

2. | Remove the front door belt inside weatherstrip (A).

3. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Front Door Latch Repair procedures

Replacement 1. Remove the front door module. (Refer to Front Door - "Front Door Module") 2. Remove the front door outside handle base (A) by pushing in the lock pins located in the back. ...

##### Front Door Side Weatherstrip Repair procedures

Replacement 1. Loosen the front door checker (B) mounting bolt. Tightening torque : 16.7 ~ 21.6 N.m (1.7 ~ 2.2 kgf.m,12.3 ~ 15.9 lb-ft) 2. Detach the clips, and then remove the front doo ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Center Fascia Panel Components and Components Location

Component Location 1. Center fascia panel ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Door Inside Handle Repair procedures

Replacement 1. Remove the rear door trim. (Refer to Rear Door - "Rear Door Trim") 2. Loosen the rear door inside handle mounting screws (A). 3. Using a flat-tip screwdriver (B), pull up the rear door inside handle lock pin (C). 4. Remove the rear door inside handle (A). 5. Inst ...
Copyright © www.ksoulev.com 2020-2021