- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Floor Console / Floor Console Assembly Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Floor Console / Floor Console Assembly Repair procedures

Replacement

Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Pull in the direction of the arrow and remove the gear knob.
Escaping power : 55± 10kgf

2. | Using a screwdriver or remover, remove the console upper cover (A).

3. | Disconnect the indicator connector (A), start/stop button switch connector (B) and multimedia jack connector (C).

4. | Press the locking pin and disconnect EPB connector.

5. | Remove the hole cover (A).

6. | Remove the console side cover (A) by pushing it backward. [LH]
When installing, insert the front of console side cover (B) to hook (A).
[RH]
When installing, insert the front of console side cover (B) to took (A).

7. | After loosening the mounting screws and bolts, remove the floor console assembly (A).

8. | Install in the reverse order of removal.
• | Make sure that the connectors are plugged in properly.
• | Replace any damaged clips.

##### Floor Console Assembly Components and Components Location

Component Location 1. Floor console assembly ...

##### Rear Console Cover Components and Components Location

Component Location 1. Rear console cover ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Virtual Engine Sound System Unit Repair procedures

Removal 1. Disconnect the negative(-) battery terminal. 2. Remove the AVN head unit. (Refer to Body Electrical System - "AVN System") 3. Disconnect the VESS unit connector (A). 4. Remove VESS unit (A) after loosening the mounting nut and screw. Installation 1. Install the VESS ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Electric Parking Brake (EPB) Repair procedures

Removal 1. Turn ignition OFF and disconnect the negative (-) battery cable. 2. Remove the floor console assembly.(Refer to Body - “Floor console assembly") 3. Disconnect the EPB control unit mounting nuts and then remove EPB control unit. Tighten torque: 3.9 ~ 5.9 N.m (0.4 ~ 0.6 ...
Copyright © www.ksoulev.com 2020-2021