- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / Main Fuse Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / Main Fuse Specifications

Specification

Item | Specification
Rated Voltage (V) | 450 (DC)
Rated Current (A) | 250 (DC)

Item | Specification | Remark
Safety Plug Cable Resistance (?) | Less than 1 (20°C) | Checkable by multi tester
Main Fuse Resistance (?) | Less than 1 (20°C) | Checkable by multi tester

##### Safety Plug Repair procedures

Inspection • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failur ...

##### Main Fuse Description and Operation

Description Installed in the safety plug, the main fuse protects the high voltage circuit from overcurrent. ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Pre-charge Relay Description and Operation

Description Installed in the Power Relay Assembly (PRA), the Pre-charge Relay connects high voltage circuit when pre-charging the inverter capacitor. When the IG is ON, the current coming through the pre-charge relay and the resistor charges the capacitor in the inverter and when the cap ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Cluster ionizer Repair procedures

Inspection 1. Press the MODE switch more than 4 times within 2 seconds while pressing the OFF switch. DisplayFail description00Normal50Cluster ion generator fault * For diagnostic procedures, refer to DTC code. Replacement 1. Disconnect the negative (-) battery terminal. 2. Remove ...
Copyright © www.ksoulev.com 2020-2021