- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Indicators And Gauges / Instrument Cluster Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Indicators And Gauges / Instrument Cluster Description and Operation

Description

Mian Features

1. | Power and charge guage
(1) | It displays the degree of economic driving by identifying the status of a driver''s operation, depending on a vehicle''s driving conditions (e.g., required power, system efficiency and charging).
(2) | It leads to economic driving by informing the driver of the optimal driving conditions depending on the vehicle''s conditions.
(3) | It displays that ECO guide and power segment will operate during driving, and also indicates the state of regenerative braking when a charge zone is instructed while driving.

2. | SOC (State Of Charge) guage
(1) | It displays the amount of charge of high-voltage battery.
(2) | It displays the charged amount of SOC received from BMS module on the digital gauge in the instrument cluster (as follows).
Display | Increase (%) | Decrease (%)
Seg0 | 0 | 0
Seg1 | 5 | 3
Seg2 | 10 | 8
Seg3 | 15 | 13
Seg4 | 20 | 18
Seg5 | 25 | 23
Seg6 | 30 | 28
Seg7 | 35 | 33
Seg8 | 40 | 38
Seg9 | 45 | 43
Seg10 | 50 | 48
Seg11 | 55 | 53
Seg12 | 60 | 58
Seg13 | 65 | 63
Seg14 | 70 | 68
Seg15 | 75 | 73
Seg16 | 80 | 78
Seg17 | 85 | 83
Seg18 | 90 | 88

3. | ECO Level Display
(1) | It displays the degree of the driver''s economic driving via ECO level.
(2) | It displays the ECO level in OLED from Steps 1 to 8.

4. | Energy Flow
(1) | It displays graphical energy flow of an EV vehicle to inform the driver of the vehicle information.
(2) | It leads to economic driving by showing the energy flow diagram by means of intuitive images.
(3) | It displays three states of energy flow of the EV vehicle graphically.
(4) | VCU module receives operation mode CAN signals to implement any relevant animation.

5. | Other indicators and warning lamps The status between C-CAN transmission modules, operating various indicator and warning lamps on the PS EV cluster, is shown. Referring to the following descriptions, any checking point or operating point can be identified in the event of inoperation of relevant function.

##### Instrument Cluster Schematic Diagrams

Circuit Diagram ...

##### Instrument Cluster Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Remove the cluster fascia panel. (Refer to Body - "Cluster Fascia Panel") 3. Remove the cluster (A) after removing screws. ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Side Impact Sensor (SIS) Repair procedures

Removal Pressure Side Impact Sensor • Removal of the airbag must be performed according to the precautions / procedures described previously. • Before disconnecting the front impact sensor connector, disconnect the front airbag connector(s). ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Ambient Temperature Sensor Repair procedures

Inspection 1. Turn the ignition switch OFF. 2. Disconnect ambient temperature sensor. 3. Check the resistance of the ambient temperature sensor between terminals 1 and 2 whether it is changed by changing of the ambient temperature. 1. Sensor Ground2. Ambient Sensor Signal Speci ...
Copyright © www.ksoulev.com 2020-2021