- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Door / Rear Door Outside Handle Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Door / Rear Door Outside Handle Repair procedures

Replacement

1. | Remove the rear door trim. (Refer to Rear Door - "Rear Door Trim")

2. | Remove the hole plug (A).

3. | After loosening the mounting bolt, remove the rear door outside handle cover (B).
Tightening torque : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)

4. | Remove the rear door outside handle (A) by sliding it backward.

5. | Install in the reverse order of removal.
• | Be sure to install the outside handle pad (A) between the outside handle and the door panel.
• | Make sure that the door locks/unlocks and opens/closes properly.

##### Rear Door Outside Handle Components and Components Location

Component Location 1. Rear door outside handle ...

##### Rear Door Latch Components and Components Location

Component Location 1. Rear door latch ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components 1. TPMS Receiver2. TPMS Sensor (FL)3. TPMS Sensor (RL)4. TPMS Sensor (RR)5. TPMS Sensor (FR) ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: ESP OFF Switch Description and Operation

Description 1. The ESP OFF switch is used by users to turn off the ESP system. 2. The ESP OFF lamp is on when ESP OFF switch is engaged. ...
Copyright © www.ksoulev.com 2020-2021