- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Panorama Sunroof / Roller Blind Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Panorama Sunroof / Roller Blind Repair procedures

Removal

1. | Open the roller blind using the panorama sunroof switch.
• | Leave 10 ~ 20cm (0.3937 ~ 0.7874 in) of the roller blind unopened.

2. | Remove the roof trim. (Refer to Roof Trim - "Roof Trim Assembly")

3. | Remove the roller blind bar (C) by pressing the top part of the lock pin (B) located on the both sides of the roller blind shoe (A).

4. | Put a fixed pin (B) into the hole located inside the groove of the right side roller blind side bracket (A). Becareful not to release tension.

5. | Remove the roller blind lower support (A) by loosening the mounting screws.

Installation

1. | Install the roller blind side bracket (A) fit into the guide groove (B).

2. | Tighten the mounting screws after installing the roller blind lower support (A).

3. | Remove the fixed pin (B) located inside the right side roller blind side bracket (A).

4. | Install the roller blind bar (A) on top of the roller blind shoe (B).

5. | Put the roller blind bar (A) into the roller blind shoe (B).

6. | Install the roof trim.

7. | Completely close the movable glass using the panorama sunroof switch.
• | Roller blind tension adjustment
(1) | Put a fixed pin (B) into the hole located inside the groove of the right side roller blind side bracket (A). Becareful not to release tension.
(2) | Remove the roller blind lower support.
(3) | Press the lock pin (A) and then remove the push the roller blind (B) in the direction of the arrow.
(4) | Remove the roller blind (A) from the roller blind support bracket (B).
(5) | Remove the fixed pin (B) from inside the groove of the right side roller blind side bracket (A).
• | Be careful not to injure your hand when the roller blind side bracket tension gets releases.
(6) | Rotate the roller fabric (B) while holding the roller fabric side bracket (A).
• | Be careful not to injure your hand when the roller blind side bracket tension gets releases.
• | Rotate it 12 times clockwise.
(7) | Put a fixed pin (B) into the hole located inside the groove of the right side roller blind side bracket (A). Becareful not to release tension.
(8) | Install the roller blind on the roller blind support bracket.

##### Panorama Sunroof Deflector Repair procedures

Replacement 1. Completely open the movable glass using the panorama sunroof switch. 2. Loosen he mounting screws (A) located at the side of the panorama sunroof deflector. ...

##### Panorama Sunroof Assembly Repair procedures

Removal • In order to remove the panorama sunroof assembly, use the tools shown in the following figure: [Tooling Diagram] Square wire Insert-type wire g ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Height Adjust Components and Components Location

Component Location 1. Height adjust ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Special Service Tools

Special Service Tools Tool Name / NumberIllustrationDescriptionHigh Voltage Power Extension Cable0K918-E4100Used for measuring the high voltage battery systemHigh Voltage Battery Check Extension Cable (21pin)0K375-E4100Used for measuring the high voltage battery systemHigh Voltage Battery Check ...
Copyright © www.ksoulev.com 2020-2021