- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Seat Belt / Front Seat Belt Buckle Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Front Seat Belt / Front Seat Belt Buckle Repair procedures

Replacement

1. | Remove the front seat assembly. (Refer to Front Seat - "Front Seat Assembly")

2. | Disconnect the front seat belt buckle connector wiring (A).

3. | After loosening the mounting bolt, remove the front seat belt buckle (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5kgf.m, 28.9 ~ 39.8 lb-ft)

4. | Install in the reverse order of removal.
• | Make sure the connector is plugged in properly.
• | Replace any damaged clips.

##### Front Seat Belt Buckle Components and Components Location

Component Location 1. Front seat belt buckle ...

##### Charge Door Opener Cover

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components Connector Pin Information No.Connector A (24 pin)Connector B (20 pin)Connector C (26 pin)Connector D (16 pin)1Battery (+)LIN (PAS)Washer motor power-2IGN 1Fuel filler (Charge door) actuator relayFront washer motor-3IGN 2LS CAN high--4Brake switchLS CAN lowMirror unfold relayMi ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Door Trim Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Be ...
Copyright © www.ksoulev.com 2020-2021