- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Power Windows / Power Window Motor Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Power Windows / Power Window Motor Repair procedures

Inspection

Front Power Window Motor

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front door trim. (Refer to Body - "Front Door Trim")

3. | Disconnect the connector (A) from the motor. (A : Safety, B : Standard)

4. | Connect the motor terminals directly to battery voltage (12V) and check that the motor operates smoothly. Next, reverse the polarity and check that the motor operates smoothly in the reverse direction. If the operation is abnormal, replace the motor. [General Window Motor]

5. | Connect the terminals No. 2 and No. 3 to battery voltage (12V) and check that the motor operates smoothly when connected to the following terminals. [Safety Window Motor]

Rear Power Window Motor

1. | Disconnect the negative (-) battery terminal.

2. | Remove the rear door trim. (Refer to Body - "Rear Door Trim")

3. | Disconnect the connector (A) from the motor.

4. | Connect the motor terminals directly to battery voltage (12V) and check that the motor operates smoothly. Next, reverse the polarity and check that the motor operates smoothly in the reverse direction. If the operation is abnormal, replace the motor.

##### Power Window Motor Components and Components Location

Components ...

##### Power Window Switch Components and Components Location

Components Driver Power Window Switch Assist Power Window Switch Rear Power Window Switch ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Tail Gate Trim Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Ta ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High voltage joint box Components and Components Location

Components Location 1. High voltage joint box2. Air conditioning compressor high voltage connector3. Electric power control unit (EPCU) high voltage cable4. On-board charger (OBC) high voltage cable connector5. PTC heater high voltage cable6. High voltage battery assembly high voltage cable7. H ...
Copyright © www.ksoulev.com 2020-2021