- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Interior Trim / Rear Transverse Trim Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Interior Trim / Rear Transverse Trim Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the trunk trim.
(1) | Remove the shelf covering (A).
(2) | Remove the luggage cover board (A).
(3) | Remove the luggage box (A).

2. | Using a clip remover, detach the rear transverse trim mounting clips (A).

3. | Using a screwdriver or remover, remove the rear transverse trim (B).

4. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Rear Transverse Trim Components and Components Location

Component Location 1. Rear transverse trim ...

##### Luggage Side Trim Components and Components Location

Component Location 1. Luggage side trim ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Reduction Gear Oil Repair procedures

Inspection 1. Lift the vehicle. 2. Remove the under cover. (Refer to Traction Motor System - "under cover") 3. Remove the oil filler plug (A). 4. Check the oil condition and then oil level (A). If the oil level is low, supplement the oil up to filler pl ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Start/Stop Button Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Remove the gear knob (A) from the console upper cover after pulling it out upward. 3. Using a screw driver or remover, remove the console upper cover (A). 4. Disconnect the indicator connector (A) and start/stop switch conne ...
Copyright © www.ksoulev.com 2020-2021