- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Fuses And Relays / ICM (Integrated Circuit Module) Relay Box Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Fuses And Relays / ICM (Integrated Circuit Module) Relay Box Repair procedures

Inspection

Normal Charge Port Relay
Check for continuity between the terminals.

1. | There should be continuity between terminals No.20 and No.10 when power and ground are connected to terminals No.10 and No.9 in the ICM-A.

Folding Motor Relay
Check for continuity between the terminals.

1. | There should be continuity between terminals No.16 and No.17 when power and ground are connected to terminals No.4 and No.8 in the ICM-A.

Unfolding Motor Relay
Check for continuity between the terminals.

1. | There should be continuity between terminals No.15 and No.17 when power and ground are connected to terminals No.6 and No.8 in the ICM-A.

##### ICM (Integrated Circuit Module) Relay Box Description and Operation

Description The ICM relay is integrated with outside mirror fold/unfold relay, front deicer relay and rear fog lamp relay and is installed inside the lower crash pad. ...

##### Hands Free System

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Crash Pad Lower Panel Components and Components Location

Component Location 1. Crash pad lower panel ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Steering Gear box Components and Components Location

Components 1. Steering Gear box ...
Copyright © www.ksoulev.com 2020-2021