- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Suspension System / Front Stabilizer Link Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Suspension System / Front Suspension System / Front Stabilizer Link Repair procedures

Replacement

1. | Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported.

2. | Remove the front wheel and tire (A) from front hub.
Tightening torque : 88.3 ~ 107.9N.m (9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft)
• | Be careful not to damage to the hub bolts when removing the front wheel and tire (A).

3. | Remove the stabilizer link (A) loosening the nut.
Tightening torque : 98.1 ~ 117.7N.m(10.0 ~ 12.0kgf.m, 72.3~86.8lb-ft)

4. | Install in the reverse order of removal.

##### Front Stabilizer Bar Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Loosen the bolt (A) and then disconnect the universal joint assembly from the pin ...

##### Sub Frame Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Loosen the bolt (A) and then disconnect the universal joint assembly from the pin ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Tail Gate Latch Components and Components Location

Component Location 1. Tail gate latch assembly ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Specifications

Specifications ItemsSpecificationsRated voltageDC 12VOperating temperature range-30°C ~ +80°C (-22 ~ +176°F)Rated loadDimmer & passing switchHigh : 1A (Relay load)Low : 1A (Relay load)Passing : 1A (Relay load)Lighting switch/ Auto lighting switch1A (Relay load)Turn signal & lane chan ...
Copyright © www.ksoulev.com 2020-2021